Software Update Notes 20240809

Preface: This only applies to devices with version numbers lower than the following. Please check the version number at T120A>Version before upgrading.




|  |  |  |  |
| --- | --- | --- | --- |
| title | content | Upgrade Content | Latest version |
| APP | Power Firmware Program | Added repair charging mode | V1.5 |
| IAP | Bottom-level upgrade program | none | V1.0 |
| LCD | Screen Display Program | Added Finnish language, optimized translation and display logic | V1.6 |

1. Use a Windows computer to download the upgrade tool and upgrade package from the following link, as shown in the figure below.

<https://www.topdon.com/pages/pro-down?fuzzy=Tornado120000>




2. Install TornadoVolt software on your computer . After the installation is complete, open the software, as shown below.



1. After turning on T120A, connect it to the computer via a USB data cable, click the Update button on the TornadoVolt software, select the upgrade package " T120A\_APP\_V1.5\_20240809.bin " on the path , and then click the Update button to upgrade. As shown below.






1. After the upgrade is complete, check the T120A APP version number. If the APP version shows V1.5, the upgrade is successful.



1. To upgrade the LCD display program, you need to install the TFTFileDownload software on your Windows computer, as shown below.





1. In the Ports position, select the interface (the content displayed on different computers is different), select the file " T120A\_LCD\_V1.6\_20240809.tft " in the Flie position, and then click the " Down " button, as shown below.



1. After the upgrade is complete, check the LCD version number of T120A. If the APP version shows V1.6, the upgrade is successful. As shown below



7. If the upgrade fails or the T120A screen displays the following information, please restart the T120A and try the upgrade again.

